|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Date |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Time |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Litres of oxygen |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Is mask fit adequate |  |  |  |  |  |  |  |  |  |  |  |  |  |
| CPAP pressure |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Oxygen saturations |  |  |  |  |  |  |  |  |  |  |  |  |  |
| RR |  |  |  |  |  |  |  |  |  |  |  |  |  |
| HR |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Note reason changes made to CPAP pressure or oxygen rate |  |  |  |  |  |  |  |  |  |  |  |  |  |
| GCS |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Filter change Y/N |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **ABG (A) CBG (C) Venous (v)** |  |  |  |  |  |  |  |  |  |  |  |  |  |
| pH |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PaC02 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Pa02 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| HC03 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Sa02 |  |  |  |  |  |  |  |  |  |  |  |  |  |

**Routine gas check not needed, but if performed please complete chart.**

**Filters should be changed every 24 hours, however more often if filter becomes visibly moist due and after in line nebuliser therapy.**